PCBA,MEGAARDUINO REV 02						
	The Android Open Source Project						
	Copyright (C) 2011						
							
ID	Description	Quantity	Ref Des	MFG	MFG P/N	Notes	
1	PCB, ASHIELD, MEGAARDUINO_REDUCED	1	N/A	N/A	N/A		
2	CAP CERM .1UF 10% 16V X7R 0603	4	C1,C2,C3,C4	AVX	0603YC104KAT2A		
3	CAP CER 22UF 10V Y5V 1206	1	C6	TDK	C3216Y5V1A226Z		
4	DIODE SWITCH LL 250V SOD-323	3	D1,D2,D3	ON SEMI	BAS21AHT1G		
5	DIODE SCHOTTKY 20V 3A SMB	1	D4	DIODES INC	B320B-13-F		
6	CONN HEADER 1x6 .100 STR 15AU	1	J1	FCI	68000-206HLF	MOUNTS ON BACK SIDE	
7	CONN HEADER 1x8 .100 STR 15AU	5	J2,J3,J4,J5,J6	FCI	68001-208HLF	MOUNTS ON BACK SIDE	
8	SW NAV JOYSTICK MOD CONTACTLESS	1	JOY1	AUSTRIAMICROSYSTEMS	N50P111		
9	RELAY PWR SPDT 1A 5VDC PCB	2	K1, K2	TE CONNECTIVITY	TSC-105L3H,000		
10	LED RED/GREEN/BLUE PLCC4 SMD	3	LED1,LED2,LED3	CREE	CLV1A-FKB-CJ1M1F1BB7R4S3		
11	LED INGAN GREEN CLEAR 0603 SMD	2	LED4,LED5	DIALIGHT	598-8081-107F		
12	IC SENSOR PHOTO ILLUMINANCE SMD	1	LS1	TOSHIBA	TPS852(T)		
13	MOSFET N-CH 50V 173MA SOT-23	2	Q1,Q2	NXP	BSN20,215		
14	TRANS NPN 40V 600MA SOT23	2	Q3,Q4	NXP	MMBT2222A,215		
15	RES 1.0K OHM 1/10W 5% 0603 SMD	6	R1,R2,R3,R4,R18,R19	PANASONIC	ERJ-3GEYJ102V		
16	RES 91 OHM 1/10W 5% 0603 SMD	6	R10,R11,R13,R14,R16,R17	PANASONIC	ERJ-3GEYJ910V		
17	RES 51K OHM 1/10W 5% 0603 SMD	1	R20	PANASONIC	ERJ-3GEYJ513V		
18	RES 10M OHM 5% 1/10W 0603 SMD	1	R21	PANASONIC	ERJ-3GEYJ106V		
19	RES 4.7K OHM 1/10W 5% 0603 SMD	5	R5,R6,R7,R8,R22	PANASONIC	ERJ-3GEYJ472V		
20	RES 150 OHM 1/10W 5% 0402 SMD	3	R9,R12,R15	PANASONIC	ERJ-3GEYJ151V		
21	SWITCH TACT 6MM 160GF H=4.3MM	4	S1,S2,S3,S4	OMRON	B3S-1000P		
22	CONN HEADER 3X 1x3 .100" STR GOLD	3	SC1	MOLEX	90120-0763	LOADED SIDE BY SIDE	
23	IC SENSOR THERMAL 3.1V TO-92-3	1	TS1	MICROCHIP TECH	MCP9701A-E/TO		
24	TERM BLOCK 6POS SIDE ENT 3.5MM	1	X2	TE CONNECTIVITY	284391-6		
25	DOC, SCHEMATIC, ASHIELD	0		N/A	N/A		
26	DOC, ASSY INSTRUCTIONS	0		N/A	N/A		
27	DOC, GERBER PACKAGE	0		N/A	N/A